**Dewalt DWS777 Specifications**

|  |  |
| --- | --- |
| Saw Blade Thickness [Metric] | **2.6 mm** |
| Blade Bore [Metric] | **30 mm** |
| Blade Speed | **6300 rpm** |
| Max. Cutting Capacity (45°/45°) [Metric] | **190 x 48 mm** |
| Max. Cutting Capacity (90°/90°) [Metric] | **270 x 60 mm** |
| Product Width [Metric] | **560 mm** |
| Max. Cutting Capacity (45°/90°) [Metric] | **190 x 60 mm** |
| Product Height [Metric] | **430 mm** |
| Product Weight [Metric] | **15.5 Kg** |
| Blade Diameter [Metric] | **216 mm** |
| Supplied in Storage Case Indicator | **No** |
| Max. Cutting Capacity (90°/45°) [Metric] | **270 x 48 mm** |
| Power Source | **Corded** |
| Power Input | **1800 W** |
| Packaging | **Carton** |
| Product Length [Metric] | **460 mm** |